







MOUNTING&WIRING

WARNING:
Improper Inst lalon my cauo electiedl shock,fre,orequpmentdmgs. The perGon perfomlng thoInstalabon must be famlar wth the constuclon  and operablon of the product and 8ssodalod hazards
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⑥Wven erir tho calng nd togln
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Wire Connection Diagram:
[image: ]

Pleeee proceed In analphabeteal order:
[image: ]A.Existing Elextrical BOX B.Crossbar C.Crossbar Scrows D.Ground Wie E.Canopy F.Wre G.Junclon Caps
atach the croasbar(B%o the existlng oleotical box(A)ualng the two crossbar scrowe(C)which are not supplied and should alresdy in
your bax.Pass the maln wie(F)and ground wre(D)through the canopy(E)and the crossber(B)unti the end of the main
wie(F)resches the cloctrical box
(A)where you can wlre use eleoticlan connedions.Be sure when
connecing the wire uso ekoctrician approved junction caps(C).stow the eXD88s wire in the electrical box(A).raise the canopy(E),aftach   canopy(Ej)o cellng.and hold the canopy(E)
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You can reduce the
drop helght of the
fuing by removing the
chaln Iinks to deslred
length
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 (
DIMMABLE:fully dimma
ble
 
with compatible dimmer
switch to create the
 
perfect
 
atmosphere
Type of Light
 
Source:
incandescent,LED or CFL
Bulbs.Bulb base
 
E12,60 watts
 
maximum(not
 
included)
)
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